{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","46.0"]
["","","Отопление","Свръх ниска","м³/мин","46.0"]
["","","","Свръх ниска","cfm","1624"]
["","","Отопление","Свръх ниска","cfm","1624"]
["Размери","Тяло","","Височина","мм","770"]
["","","","Широчина","мм","900"]
["","","","Дълбочина","мм","320"]
["Тегло","Тяло","","","kg","71"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","730"]
["","","Отопление","Свръх ниска","обор.","730"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-10"]
["","","","Макс.","°C (сух термометър)","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15"]
["","","","Макс.","°C с влажен термометър","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","52"]
["","Отопление","","Висок","дБА","52"]
["Хладилен агент","Тип","","","","R-410A"]
["","Зареждане","","","kg","2.3"]
["","Маса","","","tCO2Eq","4.8"]
["","Потенциал на глобално затопляне","","","","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","30"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","20"]
["Стандартни аксесоари","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Електрозахранване","Фаза","","","","1~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","220-240"]
["Забележки","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]