{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","47","47","48","48"]
["","Охлаждане","","Висок","дБА","46","46","48","48"]
["Стандартни аксесоари","Капачка за източващ отвор","","","","1","1","","1"]
["","Ръководство за монтаж","","","","1","1","1","1"]
["","Етикет за маса на хладилен агент","","","","1","1","1"]
["","Етикети на няколко езика за флуорираните парникови газове","","","","1","1","Етикети на няколко езика за флуорираните парникови газове"]
["Хладилен агент","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","Потенциал на глобално затопляне","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Зареждане","","","кг","1.0","1.0","1.20","1.3"]
["","Тип","","","","R-410A","R-410A","R-410A","R-410A"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","RPM","780","780","780","790"]
["","","Отопление","Свръх ниска","RPM","740","740","740","780"]
["Работен диапазон","Охлаждане","околна температура","Макс.","°CDB","46","46","46","46"]
["","","","Мин.","°CDB","-10","-10","-10","-10"]
["","Отопление","околна температура","Макс.","°C (влажен термометър)","18","18","18","18"]
["","","","Мин.","°C (влажен термометър)","-15","-15","-15","-15"]
["Тръбни съединения","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","","","15"]
["","Допълнително количество хладилен агент","","","кг/м","","","0,020 (за дължина на тръбопровод, надвишаваща 10 м)"]
["Размери","Тяло","","Широчина","mm","765","765","765","765"]
["","","","Дълбочина","mm","285","285","285","285"]
["","","","Височина","mm","550","550","550","550"]
["Компресор","Type","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Тегло","Тяло","","","кг","34","34","34","39"]
["Вентилатор","Скорост на въздушния поток","Отопление","Свръх ниска","cfm","904","904","904","960"]
["","","","Свръх ниска","м³/мин","25.6","25.6","25.6","27.2"]
["","","Охлаждане","Свръх ниска","м³/мин","30.1","30.1","30.1","30.6"]
["","","","Свръх ниска","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Съдържа флуорирани парникови газове","(4) - Съдържа флуорирани парникови газове","(4) - Съдържа флуорирани парникови газове","(4) - Съдържа флуорирани парникови газове"]
["Стандартни аксесоари","Тапа за източващ отвор","","","","","","1"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Свръх ниска","м³/мин","","","","","48.9","45.0"]
["","","Отопление","Свръх ниска","м³/мин","","","","","43.1","46.3"]
["","","","Свръх ниска","cfm","","","","","1727","1589"]
["","","Отопление","Свръх ниска","cfm","","","","","1522","1635"]
["Размери","Тяло","","Височина","mm","","","","","735","735"]
["","","","Широчина","mm","","","","","825","825"]
["","","","Дълбочина","mm","","","","","300","300"]
["Тегло","Тяло","","","кг","","","","","47","48"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","RPM","","","","","670"]
["","","Отопление","Свръх ниска","RPM","","","","","670"]
["Компресор","Тип","","","","","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","","","","","-10","-10"]
["","","","Макс.","°CDB","","","","","46","46"]
["","Отопление","околна температура","Мин.","°C (влажен термометър)","","","","","-15","-15"]
["","","","Макс.","°C (влажен термометър)","","","","","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","","","","48","49"]
["","","","Ниско","дБА","","","","","44","46"]
["","Отопление","","Висок","дБА","","","","","48","49"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","","","","45","46"]
["Хладилен агент","Тип","","","","","","","","R-410A","R-410A"]
["","Зареждане","","","кг","","","","","1.7","1.5"]
["","Маса","","","tCO2Eq","","","","","3.5","3.1"]
["","Потенциал на глобално затопляне","","","","","","","","2087.5","2087.5"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","","","","","30","30"]
["","Допълнително количество хладилен агент","","","кг/м","","","","","0,020 (за дължина на тръбопровод, надвишаваща 10 м)","0,020 (за дължина на тръбопровод, надвишаваща 10 м)"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","","","","","20.0","20"]
["Стандартни аксесоари","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Електрозахранване","Фаза","","","","","","","","1~","1~"]
["","Честота","","","Хц","","","","","50","50"]
["","Напрежение","","","V","","","","","220-230-240","220-230-240"]
["Забележки","","","","","","","","","","(1) - 230V"]