{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-N"]
[]
[]
[]
[]
["","","","","","RXTM30N2V1B","RXTM40N2V1B"]
["Ниво на звуково налягане","Отопление","","Ном.","dBA","49","49"]
["","Охлаждане","","Ном.","dBA","48","48"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1"]
["","Етикет за маса на хладилен агент","","","","1","1"]
["","Етикети на няколко езика за флуорираните парникови газове","","","","1","1"]
["Хладилен агент","Charge","","","TCO2Eq","0.7","0.7"]
["","Потенциал на глобално затопляне","","","","675","675"]
["","Количество","","","кг","1.1","1.1"]
["","Тип","","","","R-32","R-32"]
["Електромотор на вентилатор","Скорост","Охлаждане","Свръх ниска","обор.","450","360"]
["","","Отопление","Свръх ниска","обор.","360","360"]
["Тръбни съединения","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","15","15"]
["","Допълнително количество хладилен агент","","","кг/м","0,02 (за дължина на тръбопровод, надвишаваща 10 м)","0,02 (за дължина на тръбопровод, надвишаваща 10 м)"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Размери","Тяло","","Широчина","mm","763","763"]
["","","","Дълбочина","mm","312","312"]
["","","","Височина","mm","551","551"]
["Тегло","Тяло","","","кг","38","38"]
["Power supply","Фаза","","","","1~","1~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","220-240","220-240"]
["Забележки","","","","","(1) - Съдържа флуорирани парникови газове","(1) - Съдържа флуорирани парникови газове"]
["","","","","","(2) - Вж. отделния чертеж за работен диапазон","(2) - Вж. отделния чертеж за работен диапазон"]
["","","","","","(3) - Вж. отделния чертеж за електрическите схеми","(3) - Вж. отделния чертеж за електрическите схеми"]