{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B9","RXZ35NV1B","RXZ50NV1B9","RXZ50NV1B"]
["Размери","Тяло","","Височина","мм","693","693","693","693","693","693"]
["","","","Широчина","мм","795","795","795","795","795","795"]
["","","","Дълбочина","мм","300","300","300","300","300","300"]
["Тегло","Тяло","","","kg","50","50","50","50","50","50"]
["Компресор","Тип","","","","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор","Херметично запечатан люлеещ се компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-10","-10","-10","-10","-10","-10"]
["","","","Макс.","°C (сух термометър)","43","43","43","43","43","43"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-20","-20","-20","-20","-20","-20"]
["","","","Макс.","°C с влажен термометър","18","18","18","18","18","18"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","46","46","48","48","49","49"]
["","Отопление","","Висок","dBA","46","46","48","48","50","50"]
["Хладилен агент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Зареждане","","","kg","1.34","1.34","1.34","1.34","1.34","1.34"]
["","Маса","","","tCO2Eq","0.9","0.9","0.9","0.9","0.9","0.9"]
["","Потенциал на глобално затопляне","","","","675","675","675","675","675","675"]
["Тръбни съединения","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","10","10","10","10","10","10"]
["","Разлика в нивата","Вътр. у-во - Външ. у-во","Макс.","м","8","8","8","8","8","8"]
["Стандартни аксесоари","Installation manual","","","","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50","50","50"]
["","Напрежение","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]