{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Размери","Тяло","","Височина","мм","870","870"]
["","","","Широчина","мм","1,100","1,100"]
["","","","Дълбочина","мм","460","460"]
["Тегло","Тяло","","","kg","117","117"]
["Компресор","Тип","","","","Херметично запечатан спирален компресор","Херметично запечатан спирален компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°C (сух термометър)","-20","-20"]
["","","","Макс.","°C (сух термометър)","46","46"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-20","-20"]
["","","","Макс.","°C с влажен термометър","15","15"]
["Sound power level","Охлаждане","","","дБА","73","76"]
["","Отопление","","","дБА","76 (1)","79 (1)"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","53","57"]
["","Отопление","","Ном.","дБА","60","63"]
["Хладилен агент","Тип","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","Потенциал на глобално затопляне","","","","675","675"]
["Тръбни връзки","Tечност","","Вън. д.","мм","9.52","9.52"]
["","Газ","","Вън. д.","мм","22.2","22.2"]
["","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","100","100"]
["","","Система","Незареден","м","30","30"]
["","Допълнително количество хладилен агент","","","кг/м","Виж ръководство за монтаж","Виж ръководство за монтаж"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1"]
["","Общи мерки за безопасност","","","","1","1"]
["","Заключващи се връзки","","","","2","2"]
["","Отстранете етикета за флуориран газ","","","","1","1"]
["","Свързващи тръби","","","","6","6"]
["Power supply","Фаза","","","","3~","3~"]
["","Честота","","","Хц","50","50"]
["","Напрежение","","","V","380-415","380-415"]
["Ток - 50 Хц","Ампераж на максималния поток (MFA)","","","A","20","20"]
["Забележки","","","","","(1) - Съгласно ENER Lot 21","(1) - Съгласно ENER Lot 21"]