{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Размери","Тяло","","Височина","mm","1,680"]
["","","","Широчина","mm","930"]
["","","","Дълбочина","mm","765"]
["Тегло","Тяло","","","кг","183.0"]
["Компресор","Тип","","","","Херметично запечатан спирален компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","-5.0"]
["","","","Макс.","°CDB","46.0"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","-15.0"]
["","","","Макс.","°C с влажен термометър","15.0"]
["Sound power level","Охлаждане","","","дБА","78.0"]
["","Отопление","","","дБА","78.0"]
["Хладилен агент","Тип","","","","R-410A"]
["","Количество","","","кг","8.3"]
["","Потенциал на глобално затопляне","","","","2,087.5"]
["Тръбни съединения","Tечност","","Вън. д.","mm","9.52"]
["","Газ","","Вън. д.","mm","22.2"]
["","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","100"]
["","","Система","Незареден","м","30"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1"]
["","Свързващи тръби","","","","4"]
["Power supply","Фаза","","","","3N~"]
["","Честота","","","Хц","50"]
["","Напрежение","","","V","380-415"]
["Ток - 50 Хц","Ампераж на максималния поток (MFA)","","","A","25"]
["Забележки","","","","","(1) - Захранването за вътрешното устройство FDQ е отделно"]
["","","","","","(2) - Вж. отделните чертежи за електрическите схеми"]
["Размери","Тяло","","Височина","mm","","1680"]
["","","","Широчина","mm","","930"]
["","","","Дълбочина","mm","","765"]
["Тегло","Тяло","","","кг","","184.0"]
["Компресор","Тип","","","","","Херметично запечатан спирален компресор"]
["Работен диапазон","Охлаждане","околна температура","Мин.","°CDB","","-5.0"]
["","","","Макс.","°CDB","","46.0"]
["","Отопление","околна температура","Мин.","°C с влажен термометър","","-15.0"]
["","","","Макс.","°C с влажен термометър","","15.0"]
["Звукова мощност","Охлаждане","","","дБА","","78.0"]
["","Отопление","","","дБА","","78.0"]
["Хладилен агент","Зареждане","","","кг","","9.3"]
["","Потенциал на глобално затопляне","","","","","2087.5"]
["","Маса","","","tCO2Eq","","19.4"]
["Тръбни съединения","Tечност","","Вън. д.","mm","","12.70"]
["","Газ","","Вън. д.","mm","","22.2"]
["","Дължина на тръбите","Макс.","Външ. у-во - Вътр. у-во","м","","100"]
["","","Система","Незареден","м","","30"]
["Стандартни аксесоари","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Електрозахранване","Честота","","","Хц","","50"]
["Ток - 50Hz","Ампераж на максималния поток (MFA)","","","A","","25"]