{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","","44","","47"]
["","","","Ном.","dBA","","41","","44"]
["","","","Тих режим","dBA","","36","","41"]
["","","","Ниско","dBA","","38","","43"]
["","Охлаждане","","Тих режим","dBA","","36","","41"]
["","","","Ниско","dBA","","38","","43"]
["","","","Висок","dBA","","44","","47"]
["","","","Ном.","dBA","","41","","44"]
["Стандартни аксесоари","Ръководство за монтаж","","","","","Ръководство за монтаж","","Ръководство за монтаж"]
["","Ръководство за работа","","","","","Ръководство за работа","","Ръководство за работа"]
["","Винтове","","","","","Винтове","","Винтове"]
["","Шайба","","","","","Шайба","","Шайба"]
["","Безжично дистанционно управление","","","","","Безжично дистанционно управление","","Безжично дистанционно управление"]
["","Блокираща решетка на капака","","","","","Блокираща решетка на капака","","Блокираща решетка на капака"]
["","Батерия","","","","","Батерия","","Батерия"]
["Системи за управление","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Тръбни съединения","течност","","Вън. д.","mm","","9.52","","9.52"]
["","газ","","Вън. д.","mm","","15.88","","15.88"]
["","Дренаж","","","","","19.05","","19.05"]
["Консумирана мощност","Охлаждане","","Ном.","kW","","0.094","","0.137"]
["","Отопление","","Ном.","kW","","0.094","","0.137"]
["Sound power level","Охлаждане","","","dBA","","56","","60"]
["","Отопление","","","dBA","","56","","60"]
["Размери","Тяло","","Широчина","mm","","820","","820"]
["","","","Дълбочина","mm","","820","","820"]
["","","","Височина","mm","","300","","300"]
["Корпус","Material","","","","","Галванизирана стомана","","Галванизирана стомана"]
["Тегло","Тяло","","","кг","","39","","39"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","","29.2","","34.0"]
["","","","Ниско","м³/мин","","21.0","","26.3"]
["","","","Ном.","м³/мин","","24.4","","29.2"]
["","","Охлаждане","Ниско","м³/мин","","21.0","","26.3"]
["","","","Ном.","м³/мин","","24.4","","29.2"]
["","","","Висок","м³/мин","","29.2","","34.0"]
["","","","Тих режим","м³/мин","","17.6","","22.1"]
["","","Охлаждане","Тих режим","м³/мин","","17.6","","22.1"]
["Декоративен панел","Тегло","","","кг","","4","","4"]
["","Размери","","Височина","mm","","82","","82"]
["","","","Дълбочина","mm","","990","","990"]
["","","","Широчина","mm","","990","","990"]
["","Цвят","","","","","Бял","","Бял"]
["Power supply","Фаза","","","","","1~","","1~"]
["","Име","","","","","V1","","V1"]
["","Честота","","","Хц","","50","","50"]
["","Напрежение","","","V","","220-240","","220-240"]
["Вентилатор","Скорост на въздушния поток","Отопление","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","15","","22.1"]
["Входяща мощност","Отопление","","Ном.","kW","0.067","","0.137"]
["","Охлаждане","","Ном.","kW","0.067","","0.137"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Тих режим","м³/мин","15","","22.1"]
["Корпус","Материал","","","","Галванизирана стомана","","Галванизирана стомана"]
["Размери","Тяло","","Височина","mm","265","","300"]
["","","","Широчина","mm","820","","820"]
["","","","Дълбочина","mm","820","","820"]
["Тегло","Тяло","","","кг","31","","39"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","24.4","","34"]
["","","","Ном.","м³/мин","20.5","","29.2"]
["","","","Ниско","м³/мин","17.6","","26.3"]
["","","Отопление","Висок","м³/мин","24.4","","34"]
["","","","Ном.","м³/мин","20.5","","29.2"]
["","","","Ниско","м³/мин","17.6","","26.3"]
["Звукова мощност","Охлаждане","","","dBA","54","","60"]
["","Отопление","","","dBA","54","","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","41","","47"]
["","","","Ном.","dBA","38","","44"]
["","","","Ниско","dBA","35","","43"]
["","","","Тих режим","dBA","32","","41"]
["","Отопление","","Висок","dBA","41","","47"]
["","","","Ном.","dBA","38","","44"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","35","","43"]
["","","","Тих режим","dBA","32","","41"]
["Тръбни съединения","Tечност","","Вън. д.","mm","9.52","","9.52"]
["","Газ","","Вън. д.","mm","15.88","","15.88"]
["","Дренаж","","","","19.05","","19.05"]
["Декоративен панел","Размери","","Височина","mm","82","","82"]
["","","","Широчина","mm","990","","990"]
["","","","Дълбочина","mm","990","","990"]
["","Тегло","","","кг","4","","4"]
["Системи за управление","Инфрачервено дистанционно управление","","","","ARCWLA","","ARCWLA"]
["","Жично дистанционно управление","","","","ARCWB","","ARCWB"]
["Стандартни аксесоари","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Електрозахранване","Фаза","","","","1~","","1~"]
["","Честота","","","Хц","50","","50"]
["","Напрежение","","","V","220-240","","220-240"]