{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","39.0","40.0","44.0"]
["","","","Среден","dBA","34.0","34.0","34.0"]
["","","","Тих режим","dBA","21.0","21.0","22.0"]
["","","","Ниско","dBA","28.0","28.0","28.0"]
["","Охлаждане","","Среден","dBA","33.0","33.0","36.0"]
["","","","Тих режим","dBA","20.0","20.0","22.0"]
["","","","Ниско","dBA","25.0","26.0","30.0"]
["","","","Висок","dBA","39.0","40.0","45.0"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","1","1"]
["","Ръководство за работа","","","","1","1","1"]
["","Батерии","","","","1","1","1"]
["","Инфрачервено дистанционно","","","","1","1","1"]
["","Сухи батерии тип ААА","","","","2","2","2"]
["","Стойка за дистанционното","","","","1","1","1"]
["","Монтажна пластина:","","","","1","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","2","2"]
["Системи за управление","Жично дистанционно управление","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.50","9.50","9.50"]
["","Дренаж","","","","18","18","18"]
["Входяща мощност","Охлаждане","","Ном.","kW","0.023","0.023","0.040"]
["","Отопление","","Ном.","kW","0.023","0.023","0.040"]
["Звукова мощност","Охлаждане","","","dBA","53.0","54.0","59.0"]
["","Отопление","","","dBA","55.0","55.0","59.0"]
["Размери","Тяло","","Широчина","мм","770","770","770"]
["","","","Дълбочина","мм","225","225","225"]
["","","","Височина","мм","286","286","286"]
["Корпус","Цвят","","","","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","","кг","8.00","8.00","9.00"]
["Power supply","Фаза","","","","1~","1~","1~"]
["","Честота","","","Хц","50","50","50"]
["","Напрежение","","","V","220-440","220-440","220-440"]
["Входяща мощност","Охлаждане","","Ном.","kW","","","","0.029"]
["","Отопление","","Ном.","kW","","","","0.029"]
["Корпус","Цвят","","","","","","","Бяло"]
["Размери","Тяло","","Височина","мм","","","","286"]
["","","","Широчина","мм","","","","770"]
["","","","Дълбочина","мм","","","","225"]
["Тегло","Тяло","","","кг","","","","8.5"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","","","11.8"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","","","8"]
["","","","Ниско","м³/мин","","","","6.4"]
["","","","Тих режим","м³/мин","","","","4.4"]
["","","Отопление","Висок","м³/мин","","","","11.9"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","","","8.6"]
["","","Отопление","Ниско","м³/мин","","","","6.5"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","","","5.3"]
["Звукова мощност","Охлаждане","","","dBA","","","","54"]
["","Отопление","","","dBA","","","","56"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","","","","43"]
["","","","Среден","dBA","","","","34"]
["","","","Ниско","dBA","","","","27"]
["","","","Тих режим","dBA","","","","20"]
["","Отопление","","Висок","dBA","","","","40"]
["","","","Среден","dBA","","","","35"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","","","","29"]
["","","","Тих режим","dBA","","","","21"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","","","6.35"]
["","Газ","","Вън. д.","мм","","","","9.5"]
["","Дренаж","","","","","","","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","","ARC470A1"]
["","Жично дистанционно управление","","","","","","","BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Електрозахранване","Фаза","","","","","","","1~"]
["","Честота","","","Хц","","","","50"]
["","Напрежение","","","V","","","","220-440"]