{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Ниво на звуково налягане","Отопление","Висок","дБА","39"]
["","","Среден","дБА","32"]
["","","Тих режим","дБА","21"]
["","","Ниско","дБА","25"]
["","Охлаждане","Среден","дБА","32"]
["","","Тих режим","дБА","21"]
["","","Ниско","дБА","25"]
["","","Висок","дБА","39"]
["Стандартни аксесоари","Ръководство за монтаж","","","1"]
["","Ръководство за работа","","","1"]
["","Въздушен филтър","","","2"]
["","Инфрачервено дистанционно","","","1"]
["","Монтажна пластина за дистанционно","","","1"]
["","Плик за винтове","","","1"]
["","Винтов капак","","","1"]
["","Сухи батерии тип ААА","","","2"]
["","Общи мерки за безопасност","","","1"]
["Хладилен агент","Потенциал на глобално затопляне","","","675.0"]
["Системи за управление","Жично дистанционно управление","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Тръбни връзки","Tечност","Вън. д.","мм","6.35"]
["","Газ","Вън. д.","мм","9.50"]
["","Дренаж","","","18"]
["Power input","Охлаждане","Ном.","kW","0.020"]
["","Отопление","Ном.","kW","0.020"]
["Sound power level","Охлаждане","","дБА","57"]
["Размери","Тяло","Широчина","мм","798"]
["","","Дълбочина","мм","189"]
["","","Височина","мм","295"]
["Корпус","Цвят","","","Палисандър"]
["Тегло","Тяло","","kg","12"]
["Power supply","Фаза","","","1~"]
["","Честота","","Хц","50"]
["","Име","","","V1"]
["","Напрежение","","V","220-240"]