{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH16E7"]
[]
[]
[]
[]
["","","","","","ETSH16P30EF7","ETSH16P30EG7","ETSH16P50EG7","ETSH16P50EF7"]
["Корпус","Цвят","","","","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)","Чисто бяло (RAL9016) / Чисто черно (RAL9017)"]
["","Материал","","","","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен","Удароустойчив пропилен"]
["Размери","Тяло","","Височина","мм","1,892","1,892","1,910","1,910"]
["","","","Широчина","мм","594","594","792","792"]
["","","","Дълбочина","мм","644","644","817","816"]
["Тегло","Тяло","","","кг","75","75","98","98"]
["Звукова мощност","Ном.","","","дБА","45.6","45.6","45.6","45.6"]
["Ниво на звуково налягане","Ном.","","","дБА","32.8","32.8","32.8","32.8"]
["Работен диапазон","Отопление","Водна страна","Мин.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Макс.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Охлаждане","околна температура","Мин.","°C със сух термометър","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Водна страна","Мин.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Макс.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Електрозахранване","Фаза","","","","1~","1~","1~","1~"]
["","Честота","","","Хц","50","50","50","50"]
["","Напрежение","","","V","230","230","230","230"]
["Забележки","","","","","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897","(1) - Топлинни загуби съгласно EN12897"]
["","","","","","(2) - NНаправНаправете справка със схемите за работни ограничения","(2) - NНаправНаправете справка със схемите за работни ограничения","(2) - NНаправНаправете справка със схемите за работни ограничения","(2) - NНаправНаправете справка със схемите за работни ограничения"]