{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":88,"n_cols":14,"rows_kept":88,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B","FTXF20A2V1B (Archived)","FTXF20A5V1B (Archived)","FTXF25A2V1B (Archived)","FTXF25A5V1B (Archived)","FTXF35A2V1B (Archived)"]
["Ниво на звуково налягане","Отопление","","Висок","dBA","40","","","","39","39","40","40","40"]
["","","","Среден","dBA","35","","","","34","34","34","34","35"]
["","","","Тих режим","dBA","21","","","","21","21","21","21","21"]
["","","","Ниско","dBA","29","","","","28","28","28","28","29"]
["","Охлаждане","","Среден","dBA","34","","","","33","33","33","33","34"]
["","","","Тих режим","dBA","20","","","","20","20","20","20","20"]
["","","","Ниско","dBA","27","","","","25","25","26","26","27"]
["","","","Висок","dBA","43","","","","39","39","40","40","43"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","","","","1","1","1","1","1"]
["","Ръководство за работа","","","","1","","","","1","1","1","1","1"]
["","Инфрачервено дистанционно","","","","1","","","","1","1","1","1","1"]
["","Сухи батерии тип ААА","","","","2","","","","2","2","2","2","2"]
["","Стойка за дистанционното","","","","1","","","","1","1","1","1","1"]
["","Монтажна пластина:","","","","1","","","","1","1","1","1","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","","","","2","2","2","2","2"]
["Системи за управление","Wired remote control","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Тръбни съединения","Tечност","","Вън. д.","мм","6.35","","","","6.35","6.35","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","9.50","","","","9.50","9.50","9.50","9.50","9.50"]
["","Дренаж","","","","18","","","","18","18","18","18","18"]
["Консумирана мощност","Охлаждане","","Ном.","кВт","0.032","","","","0.017","0.017","0.019","0.019","0.032"]
["","Отопление","","Ном.","кВт","0.032","","","","0.020","0.020","0.020","0.020","0.032"]
["Sound power level","Охлаждане","","","dBA","58","","","","55","55","55","55","58"]
["","Отопление","","","dBA","58","","","","55","55","55","55","58"]
["Размери","Тяло","","Широчина","мм","770","","","","770","770","770","770","770"]
["","","","Дълбочина","мм","225","","","","225","225","225","225","225"]
["","","","Височина","мм","286","","","","286","286","286","286","286"]
["Корпус","Цвят","","","","Бяло","","","","Бяло","Бяло","Бяло","Бяло","Бяло"]
["Тегло","Тяло","","","кг","9.00","","","","9.00","9.00","9.00","9.00","9.00"]
["Вентилатор","Скорост на въздушния поток","Отопление","Висок","м³/мин","11.5","","","","10.3","10.3","10.3","10.3","11.5"]
["","","","Ниско","м³/мин","7.0","","","","6.5","6.5","6.7","6.7","7.0"]
["","","","Среден","м³/мин","9.0","","","","8.4","8.4","8.6","8.6","9.0"]
["","","","Тих режим","м³/мин","5.3","","","","5.3","5.3","5.3","5.3","5.3"]
["","","Охлаждане","Ниско","м³/мин","6.3","","","","5.9","5.9","6.1","6.1","6.3"]
["","","","Среден","м³/мин","8.3","","","","7.9","7.9","8.1","8.1","8.3"]
["","","","Висок","м³/мин","11.5","","","","9.8","9.8","10.1","10.1","11.5"]
["","","","Тих режим","м³/мин","4.5","","","","4.4","4.4","4.4","4.4","4.5"]
["Power supply","Фаза","","","","1~","","","","1~","1~","1~","1~","1~"]
["","Честота","","","Хц","50","","","","50","50","50","50","50"]
["","Напрежение","","","V","220-240","","","","220-240","220-240","220-240","220-240","220-240"]
["Входяща мощност","Охлаждане","","Ном.","кВт","","0.029","0.032","0.032"]
["","Отопление","","Ном.","кВт","","0.032","0.035","0.035"]
["Корпус","Цвят","","","","","Бяло","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","","295","295","295"]
["","","","Широчина","мм","","990","990","990"]
["","","","Дълбочина","мм","","263","263","263"]
["Тегло","Тяло","","","кг","","13.5","13.5","13.5"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","16.8","17.3","17.3"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","14.4","14.8","14.8"]
["","","","Ниско","м³/мин","","11.9","12.2","12.2"]
["","","","Тих режим","м³/мин","","10.5","10.7","10.7"]
["","","Отопление","Висок","м³/мин","","17.3","17.9","17.9"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","14.8","15.8","15.8"]
["","","Отопление","Ниско","м³/мин","","12.2","12.8","12.8"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","10.7","11.3","11.3"]
["Звукова мощност","Охлаждане","","","dBA","","59","60","62"]
["","Отопление","","","dBA","","61","62","62"]
["Ниво на звуково налягане","Охлаждане","","Висок","dBA","","43","45","46"]
["","","","Среден","dBA","","39","41","42"]
["","","","Ниско","dBA","","34","36","37"]
["","","","Тих режим","dBA","","31","33","34"]
["","Отопление","","Висок","dBA","","42","44","45"]
["","","","Среден","dBA","","38","40","41"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","dBA","","33","35","36"]
["","","","Тих режим","dBA","","30","32","33"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","","12.7","12.7","12.7"]
["","Дренаж","","","","","18","18","18"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Жично дистанционно управление","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Стандартни аксесоари","Installation manual","","","","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2"]
["","Operation manual","","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","2","2"]
["","Indoor unit fixing screws","","","","","2","2","2"]
["","Infrared remote control","","","","","1","1","1"]
["","Mounting plate","","","","","1","1","1"]
["","Remote control holder","","","","","1","1","1"]
["Електрозахранване","Име","","","","","V1","V1","V1"]
["","Фаза","","","","","1~","1~","1~"]
["","Честота","","","Хц","","50","50","50"]
["","Напрежение","","","V","","220-240","220-240","220-240"]