{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Ниво на звуково налягане","Отопление","Висок","дБА","47","47"]
["","","Тих режим","дБА","19","19"]
["","","Ниско","дБА","23","23"]
["","Охлаждане","Тих режим","дБА","21","21"]
["","","Ниско","дБА","33","33"]
["","","Висок","дБА","45","45"]
["","","Ном.","дБА","37","36"]
["","Охлаждане","Ном.","дБА","39","39"]
["Стандартни аксесоари","Ръководство за монтаж","","","1","1"]
["","Ръководство за работа","","","1","1"]
["","Инфрачервено дистанционно","","","1","1"]
["","Батерии","","","2","2"]
["","Стойка за дистанционното","","","1","1"]
["","Монтажна пластина:","","","1","1"]
["","Филтър за фотокаталитично пречистване на въздуха от титанов апатит","","","2","2"]
["","Фиксиращи винтове за вътрешното устройство","","","2","2"]
["Системи за управление","Infrared remote control","","","ARC466A9","ARC466A9"]
["Тръбни връзки","Tечност","Вън. д.","мм","6.35","6.35"]
["","Газ","Вън. д.","мм","9.5","9.5"]
["","Дренаж","","","18","18"]
["Power input","Охлаждане","Ном.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Отопление","Ном.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Охлаждане","","дБА","59","59"]
["","Отопление","","дБА","62","62"]
["Размери","Тяло","Широчина","мм","900","900"]
["","","Дълбочина","мм","215","215"]
["","","Височина","мм","298","298"]
["Корпус","Цвят","","","Бяло","Бяло"]
["Тегло","Тяло","","kg","12","12"]
["Power supply","Фаза","","","1~","1~"]
["","Честота","","Хц","50","50"]
["","Име","","","V1","V1"]
["","Напрежение","","V","220-240","220-240"]
["Забележки","","","","(1) - Когато свързвате с мулти-системно външно устройство, консултирайте се със спецификациите за мулти-външното устройство за свързване","(1) - Когато свързвате с мулти-системно външно устройство, консултирайте се със спецификациите за мулти-външното устройство за свързване"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]