{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Ниво на звуково налягане","Отопление","","Висок","дБА","40","","","","","","45"]
["","","","Тих режим","дБА","19","","","","","","22"]
["","","","Ниско","дБА","27","","","","","","33"]
["","Охлаждане","","Тих режим","дБА","19","","","","","","21"]
["","","","Ниско","дБА","24","","","","","","33"]
["","","","Висок","дБА","40","","","","","","45"]
["","","","Ном.","дБА","34","","","","","","39"]
["","Охлаждане","","Ном.","дБА","32","","","","","","39"]
["Стандартни аксесоари","Ръководство за монтаж","","","","1","","","","","","1"]
["","Ръководство за работа","","","","1","","","","","","1"]
["","Безжично дистанционно управление","","","","1","","","","","","1"]
["","Батерии","","","","2","","","","","","2"]
["","Стойка за дистанционното","","","","1","","","","","","1"]
["","Монтажна пластина:","","","","1","","","","","","1"]
["","Фиксиращи винтове за вътрешното устройство","","","","2","","","","","","2"]
["","Филтър за фотокаталитично пречистване на въздуха от титанов апатит","","","","2","","","","","","2"]
["Системи за управление","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Тръбни връзки","Tечност","","Вън. д.","мм","6.35","","","","","","6.35"]
["","Газ","","Вън. д.","мм","9.5","","","","","","9.5"]
["","Дренаж","","","","18","","","","","","18"]
["Power input","Охлаждане","","Ном.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Отопление","","Ном.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Охлаждане","","","дБА","58","","","","","","59"]
["","Отопление","","","дБА","58","","","","","","59"]
["Размери","Тяло","","Широчина","мм","780","","","","","","900"]
["","","","Дълбочина","мм","215","","","","","","215"]
["","","","Височина","мм","289","","","","","","298"]
["Корпус","Цвят","","","","Бяло","","","","","","Бяло"]
["Тегло","Тяло","","","kg","8","","","","","","11"]
["Power supply","Фаза","","","","1~","","","","","","1~"]
["","Честота","","","Хц","50","","","","","","50"]
["","Име","","","","V1","","","","","","V1"]
["","Напрежение","","","V","220-240","","","","","","220-240"]
["Забележки","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Когато свързвате с мулти-системно външно устройство, консултирайте се със спецификациите за мулти-външното устройство за свързване","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Входяща мощност","Охлаждане","","Ном.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Отопление","","Ном.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Корпус","Цвят","","","","","Бяло","Бяло","Бяло","Бяло","Бяло","","Бяло","Бяло","Бяло"]
["Размери","Тяло","","Височина","мм","","215","289","215","298","215","","215","298","215"]
["","","","Широчина","мм","","780","780","780","900","900","","900","900","900"]
["","","","Дълбочина","мм","","289","215","289","215","298","","298","215","298"]
["Тегло","Тяло","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Висок","м³/мин","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Дебит на въздушен поток","Охлаждане","Среден","м³/мин","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Ниско","м³/мин","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Тих режим","м³/мин","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Отопление","Висок","м³/мин","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Дебит на въздушен поток","Отопление","Среден","м³/мин","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Отопление","Ниско","м³/мин","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Вентилатор-=-Скорост на въздушния поток-=-Отопление-=-Тих режим-=-м³/мин","м³/мин","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Звукова мощност","Охлаждане","","","дБА","","58","58","58","59","59","","59","60","60"]
["","Отопление","","","дБА","","58","58","58","59","59","","59","60","60"]
["Ниво на звуково налягане","Охлаждане","","Висок","дБА","","40","41","41","45","45","","45","46","46"]
["","","","Среден","дБА","","32","33","33","","37","","39","","40"]
["","","","Ниско","дБА","","24","25","25","29","29","","33","34","34"]
["","","","Тих режим","дБА","","19","19","19","19","19","","21","23","23"]
["","Отопление","","Висок","дБА","","40","41","41","45","45","","45","47","47"]
["","","","Среден","дБА","","34","34","34","","39","","39","","40"]
["","","","Ниво на звуково налягане-=-Отопление-=-Ниско-=-dBA","дБА","","27","27","27","29","29","","33","34","34"]
["","","","Тих режим","дБА","","19","19","19","19","19","","22","24","24"]
["Тръбни съединения","Tечност","","Вън. д.","мм","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Газ","","Вън. д.","мм","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Дренаж","","","","","18","18","18","18","18","","18","18","18"]
["Системи за управление","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Стандартни аксесоари","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Електрозахранване","Име","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Фаза","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Честота","","","Хц","","50","50","50","50","50","","50","50","50"]
["","Напрежение","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Вентилатор","Скорост на въздушния поток","Охлаждане","Ном.","м³/мин","","","9.1","","11.2","","","","11.9"]
["Ниво на звуково налягане","Охлаждане","","Ном.","дБА","","","33","","37","","","","40"]
["Вентилатор","Скорост на въздушния поток","Отопление","Ном.","м³/мин","","","8.0","","9.3","","","","10.8"]
["Ниво на звуково налягане","Отопление","","Ном.","дБА","","","34","","39","","","","40"]
["Системи за управление","Инфрачервено дистанционно управление","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Стандартни аксесоари","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Забележки","","","","","","","","","","","(4) - 240V"]